**GORE® GR Sheet Gasketing**

Exceptionally resistant to creep, cold flow and aggressive media, this 100% ePTFE gasket sheet reliably seals steel piping and equipment. GORE® GR Sheet Gasketing is stronger and more dimensionally stable than other ePTFE gaskets and a versatile, single-solution material for both standard and custom gasketing shapes and sizes.

**GORE® Universal Pipe Gasket (Style 800)**

Reliably seal a broad range of flange materials with this low stress-to-seal, exceptionally dimensionally stable and chemically resistant 100% ePTFE gasket.  
This single gasket solution can reduce the process safety and production downtime risks caused by the use of an incorrect gasket material.

**GORE® Gasket Tape Series 500**

This exceptionally creep resistant 100% ePTFE form-in-place gasket tape delivers worry-free sealing performance for large steel flanges. It forms to fit any shape, instantly. It is so easy to handle and install, that even large flanges are a one-person job. GORE Gasket Tape Series 500 is also highly conformable, compensating for considerable flange irregularities.

**GORE® Gasket Tape Series 1000**

GORE® Gasket Tape Series 1000 addresses all the challenges of reliably sealing large glass-lined steel flanges. Made of 100 % expanded PTFE, this highly conformable tape is chemically inert, and highly resistant to creep, cold flow and clamp-force loss. Its proprietary barrier core maintains an extra tight seal even at low loads.

**GORE® Joint Sealant**

Versatile and easy-to-install, this 100% ePTFE sealing cord is a cost-effective solution for large steel flanges in general-use applications. It is the standard sealing material for many MRO (Maintenance, Repair and Operations) teams because it seals reliably and it is easy and cost-effective to install – particularly on rectangular or irregular shapes, and rough or pitted surfaces.